Orcad to eeschema converter (tested only under Orcad SDT386 files)
liborcad2eeschema is the Orcad library to eeschema library converter
Usage:
1 decompile Orcad library file ( i.e. convert it to is ascii form).
	Usualy the Orcad lib is something as file.lib and is decompiled form is file.src
2 Run liborcad2eeschema.exe with the two args <file.src> <libeeschema.lib>, i.e.:
	liborcad2eeschema.exe file.src libeeschema.lib
	
orc2eeschema.exe is the Orcad Schematic to eschema schematic converter
1 Create an library archive (with Orcad Libarch) (something as mylibarch.src)
2 Convert Orcad Schematic to .aex form( exchange form)
3 for each .aex file run
	orc2eeschema.exe <source orcad> <output eeschema> <mylibarch> (with no extension for filenames)

4 - Add mylibarch.lib to eeschema list libraries (in first position)

5 - Global Labels must be adjusted in eeschema.
